Issued to:		FUZHOU AOK LED LIGHT CO LTD  	
		FLOOR 3 BUILDING 23
NO. 152 GUANPU RD
CANGSHAN DISTRICT
FUZHOU
FUJIAN 350008 CHINA	
			
This is to certify that
representative samples of		LIGHT-EMITTING-DIODE SURFACE-MOUNTED LUMINAIRES	
		LED Surface Mounted Luminaire - AOK-YYWiE-NV-XX-XX-XXXX-BN-P.
Where "YYW" stands for input wattage and can be 18W, 26W, 35W, 55W, 72W, 82W, 110W, 115W, 150W, 190W, 200W, or 260W. First "XX" stands for brand of LED and can be any letters or digits. Second "XX" stands for assembly of photocontrol and can be 00 or PH. "XXXX" stands for color temperature of LED and color rendering index and can be any letters or digits. "BN" stands for beam angles and can be any letters or digits. "P" stands for mounting means and can be "A"	
			
		Have been investigated by UL in accordance with the Standard(s) indicated on this Certificate.	
			
Standard(s) for Safety:		See Next Page	
Additional Information:		See the UL Online Certifications Directory at www.ul.com/database for additional information	

Only those products bearing the UL Certification Mark should be considered as being covered by UL's Certification and Follow-Up Service.

Look for the UL Certification Mark on the product.

This is to certify that representative samples of the product as specified on this certificate were tested according to the current UL requirements.

Standards:

UL 1598 - Luminaires
CSA C22.2 No. 250.0-08 - Luminaires
UL 8750 - Light Emitting Diode (LED)
Equipment for Use in Lighting Products
CAN/CSA C22.2 No. 250.13-14 - Light Emitting Diode (LED) Equipment for Lighting Applications